


ARM Macro Assembler    Page 1 


    1 00000000         ;*******************************************************
                       ************************
    2 00000000         ;* File Name          : startup_stm32f030x8.s
    3 00000000         ;* Author             : MCD Application Team
    4 00000000         ;* Description        : STM32F030x8 devices vector table
                        for MDK-ARM toolchain.
    5 00000000         ;*                      This module performs:
    6 00000000         ;*                      - Set the initial SP
    7 00000000         ;*                      - Set the initial PC == Reset_Ha
                       ndler
    8 00000000         ;*                      - Set the vector table entries w
                       ith the exceptions ISR address
    9 00000000         ;*                      - Branches to __main in the C li
                       brary (which eventually
   10 00000000         ;*                        calls main()).
   11 00000000         ;*                      After Reset the CortexM0 process
                       or is in Thread mode,
   12 00000000         ;*                      priority is Privileged, and the 
                       Stack is set to Main.
   13 00000000         ;*******************************************************
                       ************************
   14 00000000         ;* @attention
   15 00000000         ;*
   16 00000000         ;* Copyright (c) 2016 STMicroelectronics.
   17 00000000         ;* All rights reserved.
   18 00000000         ;*
   19 00000000         ;* This software is licensed under terms that can be fou
                       nd in the LICENSE file
   20 00000000         ;* in the root directory of this software component.
   21 00000000         ;* If no LICENSE file comes with this software, it is pr
                       ovided AS-IS.
   22 00000000         ;*
   23 00000000         ;*******************************************************
                       ************************
   24 00000000         ;* <<< Use Configuration Wizard in Context Menu >>>
   25 00000000         ;
   26 00000000         
   27 00000000         ; Amount of memory (in bytes) allocated for Stack
   28 00000000         ; Tailor this value to your application needs
   29 00000000         ; <h> Stack Configuration
   30 00000000         ;   <o> Stack Size (in Bytes) <0x0-0xFFFFFFFF:8>
   31 00000000         ; </h>
   32 00000000         
   33 00000000 00000400 
                       Stack_Size
                               EQU              0x400
   34 00000000         
   35 00000000                 AREA             STACK, NOINIT, READWRITE, ALIGN
=3
   36 00000000         Stack_Mem
                               SPACE            Stack_Size
   37 00000400         __initial_sp
   38 00000400         
   39 00000400         
   40 00000400         ; <h> Heap Configuration
   41 00000400         ;   <o>  Heap Size (in Bytes) <0x0-0xFFFFFFFF:8>
   42 00000400         ; </h>
   43 00000400         
   44 00000400 00000200 



ARM Macro Assembler    Page 2 


                       Heap_Size
                               EQU              0x200
   45 00000400         
   46 00000400                 AREA             HEAP, NOINIT, READWRITE, ALIGN=
3
   47 00000000         __heap_base
   48 00000000         Heap_Mem
                               SPACE            Heap_Size
   49 00000200         __heap_limit
   50 00000200         
   51 00000200                 PRESERVE8
   52 00000200                 THUMB
   53 00000200         
   54 00000200         
   55 00000200         ; Vector Table Mapped to Address 0 at Reset
   56 00000200                 AREA             RESET, DATA, READONLY
   57 00000000                 EXPORT           __Vectors
   58 00000000                 EXPORT           __Vectors_End
   59 00000000                 EXPORT           __Vectors_Size
   60 00000000         
   61 00000000 00000000 
                       __Vectors
                               DCD              __initial_sp ; Top of Stack
   62 00000004 00000000        DCD              Reset_Handler ; Reset Handler
   63 00000008 00000000        DCD              NMI_Handler ; NMI Handler
   64 0000000C 00000000        DCD              HardFault_Handler ; Hard Fault 
                                                            Handler
   65 00000010 00000000        DCD              0           ; Reserved
   66 00000014 00000000        DCD              0           ; Reserved
   67 00000018 00000000        DCD              0           ; Reserved
   68 0000001C 00000000        DCD              0           ; Reserved
   69 00000020 00000000        DCD              0           ; Reserved
   70 00000024 00000000        DCD              0           ; Reserved
   71 00000028 00000000        DCD              0           ; Reserved
   72 0000002C 00000000        DCD              SVC_Handler ; SVCall Handler
   73 00000030 00000000        DCD              0           ; Reserved
   74 00000034 00000000        DCD              0           ; Reserved
   75 00000038 00000000        DCD              PendSV_Handler ; PendSV Handler
                                                            
   76 0000003C 00000000        DCD              SysTick_Handler 
                                                            ; SysTick Handler
   77 00000040         
   78 00000040         ; External Interrupts
   79 00000040 00000000        DCD              WWDG_IRQHandler 
                                                            ; Window Watchdog
   80 00000044 00000000        DCD              0           ; Reserved
   81 00000048 00000000        DCD              RTC_IRQHandler ; RTC through EX
                                                            TI Line
   82 0000004C 00000000        DCD              FLASH_IRQHandler ; FLASH
   83 00000050 00000000        DCD              RCC_IRQHandler ; RCC
   84 00000054 00000000        DCD              EXTI0_1_IRQHandler 
                                                            ; EXTI Line 0 and 1
                                                            
   85 00000058 00000000        DCD              EXTI2_3_IRQHandler 
                                                            ; EXTI Line 2 and 3
                                                            
   86 0000005C 00000000        DCD              EXTI4_15_IRQHandler 
                                                            ; EXTI Line 4 to 15
                                                            



ARM Macro Assembler    Page 3 


   87 00000060 00000000        DCD              0           ; Reserved
   88 00000064 00000000        DCD              DMA1_Channel1_IRQHandler 
                                                            ; DMA1 Channel 1
   89 00000068 00000000        DCD              DMA1_Channel2_3_IRQHandler ; DM
                                                            A1 Channel 2 and Ch
                                                            annel 3
   90 0000006C 00000000        DCD              DMA1_Channel4_5_IRQHandler ; DM
                                                            A1 Channel 4 and Ch
                                                            annel 5
   91 00000070 00000000        DCD              ADC1_IRQHandler ; ADC1 
   92 00000074 00000000        DCD              TIM1_BRK_UP_TRG_COM_IRQHandler 
                                                            ; TIM1 Break, Updat
                                                            e, Trigger and Comm
                                                            utation
   93 00000078 00000000        DCD              TIM1_CC_IRQHandler ; TIM1 Captu
                                                            re Compare
   94 0000007C 00000000        DCD              0           ; Reserved
   95 00000080 00000000        DCD              TIM3_IRQHandler ; TIM3
   96 00000084 00000000        DCD              TIM6_IRQHandler ; TIM6
   97 00000088 00000000        DCD              0           ; Reserved
   98 0000008C 00000000        DCD              TIM14_IRQHandler ; TIM14
   99 00000090 00000000        DCD              TIM15_IRQHandler ; TIM15
  100 00000094 00000000        DCD              TIM16_IRQHandler ; TIM16
  101 00000098 00000000        DCD              TIM17_IRQHandler ; TIM17
  102 0000009C 00000000        DCD              I2C1_IRQHandler ; I2C1
  103 000000A0 00000000        DCD              I2C2_IRQHandler ; I2C2
  104 000000A4 00000000        DCD              SPI1_IRQHandler ; SPI1
  105 000000A8 00000000        DCD              SPI2_IRQHandler ; SPI2
  106 000000AC 00000000        DCD              USART1_IRQHandler ; USART1
  107 000000B0 00000000        DCD              USART2_IRQHandler ; USART2
  108 000000B4         
  109 000000B4         __Vectors_End
  110 000000B4         
  111 000000B4 000000B4 
                       __Vectors_Size
                               EQU              __Vectors_End - __Vectors
  112 000000B4         
  113 000000B4                 AREA             |.text|, CODE, READONLY
  114 00000000         
  115 00000000         ; Reset handler routine
  116 00000000         Reset_Handler
                               PROC
  117 00000000                 EXPORT           Reset_Handler                 [
WEAK]
  118 00000000                 IMPORT           __main
  119 00000000                 IMPORT           SystemInit
  120 00000000 4807            LDR              R0, =SystemInit
  121 00000002 4780            BLX              R0
  122 00000004 4807            LDR              R0, =__main
  123 00000006 4700            BX               R0
  124 00000008                 ENDP
  125 00000008         
  126 00000008         ; Dummy Exception Handlers (infinite loops which can be 
                       modified)
  127 00000008         
  128 00000008         NMI_Handler
                               PROC
  129 00000008                 EXPORT           NMI_Handler                    
[WEAK]



ARM Macro Assembler    Page 4 


  130 00000008 E7FE            B                .
  131 0000000A                 ENDP
  133 0000000A         HardFault_Handler
                               PROC
  134 0000000A                 EXPORT           HardFault_Handler              
[WEAK]
  135 0000000A E7FE            B                .
  136 0000000C                 ENDP
  137 0000000C         SVC_Handler
                               PROC
  138 0000000C                 EXPORT           SVC_Handler                    
[WEAK]
  139 0000000C E7FE            B                .
  140 0000000E                 ENDP
  141 0000000E         PendSV_Handler
                               PROC
  142 0000000E                 EXPORT           PendSV_Handler                 
[WEAK]
  143 0000000E E7FE            B                .
  144 00000010                 ENDP
  145 00000010         SysTick_Handler
                               PROC
  146 00000010                 EXPORT           SysTick_Handler                
[WEAK]
  147 00000010 E7FE            B                .
  148 00000012                 ENDP
  149 00000012         
  150 00000012         Default_Handler
                               PROC
  151 00000012         
  152 00000012                 EXPORT           WWDG_IRQHandler                
[WEAK]
  153 00000012                 EXPORT           RTC_IRQHandler                 
[WEAK]
  154 00000012                 EXPORT           FLASH_IRQHandler               
[WEAK]
  155 00000012                 EXPORT           RCC_IRQHandler                 
[WEAK]
  156 00000012                 EXPORT           EXTI0_1_IRQHandler             
[WEAK]
  157 00000012                 EXPORT           EXTI2_3_IRQHandler             
[WEAK]
  158 00000012                 EXPORT           EXTI4_15_IRQHandler            
[WEAK]
  159 00000012                 EXPORT           DMA1_Channel1_IRQHandler       
[WEAK]
  160 00000012                 EXPORT           DMA1_Channel2_3_IRQHandler     
[WEAK]
  161 00000012                 EXPORT           DMA1_Channel4_5_IRQHandler     
[WEAK]
  162 00000012                 EXPORT           ADC1_IRQHandler                
[WEAK]
  163 00000012                 EXPORT           TIM1_BRK_UP_TRG_COM_IRQHandler 
[WEAK]
  164 00000012                 EXPORT           TIM1_CC_IRQHandler             
[WEAK]
  165 00000012                 EXPORT           TIM3_IRQHandler                
[WEAK]
  166 00000012                 EXPORT           TIM6_IRQHandler                



ARM Macro Assembler    Page 5 


[WEAK]
  167 00000012                 EXPORT           TIM14_IRQHandler               
[WEAK]
  168 00000012                 EXPORT           TIM15_IRQHandler               
[WEAK]
  169 00000012                 EXPORT           TIM16_IRQHandler               
[WEAK]
  170 00000012                 EXPORT           TIM17_IRQHandler               
[WEAK]
  171 00000012                 EXPORT           I2C1_IRQHandler                
[WEAK]
  172 00000012                 EXPORT           I2C2_IRQHandler                
[WEAK]
  173 00000012                 EXPORT           SPI1_IRQHandler                
[WEAK]
  174 00000012                 EXPORT           SPI2_IRQHandler                
[WEAK]
  175 00000012                 EXPORT           USART1_IRQHandler              
[WEAK]
  176 00000012                 EXPORT           USART2_IRQHandler              
[WEAK]
  177 00000012         
  178 00000012         
  179 00000012         WWDG_IRQHandler
  180 00000012         RTC_IRQHandler
  181 00000012         FLASH_IRQHandler
  182 00000012         RCC_IRQHandler
  183 00000012         EXTI0_1_IRQHandler
  184 00000012         EXTI2_3_IRQHandler
  185 00000012         EXTI4_15_IRQHandler
  186 00000012         DMA1_Channel1_IRQHandler
  187 00000012         DMA1_Channel2_3_IRQHandler
  188 00000012         DMA1_Channel4_5_IRQHandler
  189 00000012         ADC1_IRQHandler
  190 00000012         TIM1_BRK_UP_TRG_COM_IRQHandler
  191 00000012         TIM1_CC_IRQHandler
  192 00000012         TIM3_IRQHandler
  193 00000012         TIM6_IRQHandler
  194 00000012         TIM14_IRQHandler
  195 00000012         TIM15_IRQHandler
  196 00000012         TIM16_IRQHandler
  197 00000012         TIM17_IRQHandler
  198 00000012         I2C1_IRQHandler
  199 00000012         I2C2_IRQHandler
  200 00000012         SPI1_IRQHandler
  201 00000012         SPI2_IRQHandler
  202 00000012         USART1_IRQHandler
  203 00000012         USART2_IRQHandler
  204 00000012         
  205 00000012 E7FE            B                .
  206 00000014         
  207 00000014                 ENDP
  208 00000014         
  209 00000014                 ALIGN
  210 00000014         
  211 00000014         ;*******************************************************
                       ************************
  212 00000014         ; User Stack and Heap initialization
  213 00000014         ;*******************************************************



ARM Macro Assembler    Page 6 


                       ************************
  214 00000014                 IF               :DEF:__MICROLIB
  221 00000014         
  222 00000014                 IMPORT           __use_two_region_memory
  223 00000014                 EXPORT           __user_initial_stackheap
  224 00000014         
  225 00000014         __user_initial_stackheap
  226 00000014         
  227 00000014 4804            LDR              R0, =  Heap_Mem
  228 00000016 4905            LDR              R1, =(Stack_Mem + Stack_Size)
  229 00000018 4A05            LDR              R2, = (Heap_Mem +  Heap_Size)
  230 0000001A 4B06            LDR              R3, = Stack_Mem
  231 0000001C 4770            BX               LR
  232 0000001E         
  233 0000001E 00 00           ALIGN
  234 00000020         
  235 00000020                 ENDIF
  236 00000020         
  237 00000020                 END
              00000000 
              00000000 
              00000000 
              00000400 
              00000200 
              00000000 
Command Line: --debug --xref --diag_suppress=9931 --cpu=Cortex-M0 --apcs=interw
ork --depend="esf drive stm32 uid\startup_stm32f030x8.d" -o"esf drive stm32 uid
\startup_stm32f030x8.o" -I.\RTE\_ESF_Drive_STM32_UID -IC:\Keil_v5\ARM\PACK\ARM\
CMSIS\5.3.0\CMSIS\Include -IC:\Keil_v5\ARM\PACK\Keil\STM32F0xx_DFP\2.1.1\Driver
s\CMSIS\Device\ST\STM32F0xx\Include --predefine="__UVISION_VERSION SETA 525" --
predefine="_RTE_ SETA 1" --predefine="STM32F030x8 SETA 1" --list=startup_stm32f
030x8.lst startup_stm32f030x8.s



ARM Macro Assembler    Page 1 Alphabetic symbol ordering
Relocatable symbols

STACK 00000000

Symbol: STACK
   Definitions
      At line 35 in file startup_stm32f030x8.s
   Uses
      None
Comment: STACK unused
Stack_Mem 00000000

Symbol: Stack_Mem
   Definitions
      At line 36 in file startup_stm32f030x8.s
   Uses
      At line 228 in file startup_stm32f030x8.s
      At line 230 in file startup_stm32f030x8.s

__initial_sp 00000400

Symbol: __initial_sp
   Definitions
      At line 37 in file startup_stm32f030x8.s
   Uses
      At line 61 in file startup_stm32f030x8.s
Comment: __initial_sp used once
3 symbols



ARM Macro Assembler    Page 1 Alphabetic symbol ordering
Relocatable symbols

HEAP 00000000

Symbol: HEAP
   Definitions
      At line 46 in file startup_stm32f030x8.s
   Uses
      None
Comment: HEAP unused
Heap_Mem 00000000

Symbol: Heap_Mem
   Definitions
      At line 48 in file startup_stm32f030x8.s
   Uses
      At line 227 in file startup_stm32f030x8.s
      At line 229 in file startup_stm32f030x8.s

__heap_base 00000000

Symbol: __heap_base
   Definitions
      At line 47 in file startup_stm32f030x8.s
   Uses
      None
Comment: __heap_base unused
__heap_limit 00000200

Symbol: __heap_limit
   Definitions
      At line 49 in file startup_stm32f030x8.s
   Uses
      None
Comment: __heap_limit unused
4 symbols



ARM Macro Assembler    Page 1 Alphabetic symbol ordering
Relocatable symbols

RESET 00000000

Symbol: RESET
   Definitions
      At line 56 in file startup_stm32f030x8.s
   Uses
      None
Comment: RESET unused
__Vectors 00000000

Symbol: __Vectors
   Definitions
      At line 61 in file startup_stm32f030x8.s
   Uses
      At line 57 in file startup_stm32f030x8.s
      At line 111 in file startup_stm32f030x8.s

__Vectors_End 000000B4

Symbol: __Vectors_End
   Definitions
      At line 109 in file startup_stm32f030x8.s
   Uses
      At line 58 in file startup_stm32f030x8.s
      At line 111 in file startup_stm32f030x8.s

3 symbols



ARM Macro Assembler    Page 1 Alphabetic symbol ordering
Relocatable symbols

.text 00000000

Symbol: .text
   Definitions
      At line 113 in file startup_stm32f030x8.s
   Uses
      None
Comment: .text unused
ADC1_IRQHandler 00000012

Symbol: ADC1_IRQHandler
   Definitions
      At line 189 in file startup_stm32f030x8.s
   Uses
      At line 91 in file startup_stm32f030x8.s
      At line 162 in file startup_stm32f030x8.s

DMA1_Channel1_IRQHandler 00000012

Symbol: DMA1_Channel1_IRQHandler
   Definitions
      At line 186 in file startup_stm32f030x8.s
   Uses
      At line 88 in file startup_stm32f030x8.s
      At line 159 in file startup_stm32f030x8.s

DMA1_Channel2_3_IRQHandler 00000012

Symbol: DMA1_Channel2_3_IRQHandler
   Definitions
      At line 187 in file startup_stm32f030x8.s
   Uses
      At line 89 in file startup_stm32f030x8.s
      At line 160 in file startup_stm32f030x8.s

DMA1_Channel4_5_IRQHandler 00000012

Symbol: DMA1_Channel4_5_IRQHandler
   Definitions
      At line 188 in file startup_stm32f030x8.s
   Uses
      At line 90 in file startup_stm32f030x8.s
      At line 161 in file startup_stm32f030x8.s

Default_Handler 00000012

Symbol: Default_Handler
   Definitions
      At line 150 in file startup_stm32f030x8.s
   Uses
      None
Comment: Default_Handler unused
EXTI0_1_IRQHandler 00000012

Symbol: EXTI0_1_IRQHandler
   Definitions
      At line 183 in file startup_stm32f030x8.s
   Uses
      At line 84 in file startup_stm32f030x8.s



ARM Macro Assembler    Page 2 Alphabetic symbol ordering
Relocatable symbols

      At line 156 in file startup_stm32f030x8.s

EXTI2_3_IRQHandler 00000012

Symbol: EXTI2_3_IRQHandler
   Definitions
      At line 184 in file startup_stm32f030x8.s
   Uses
      At line 85 in file startup_stm32f030x8.s
      At line 157 in file startup_stm32f030x8.s

EXTI4_15_IRQHandler 00000012

Symbol: EXTI4_15_IRQHandler
   Definitions
      At line 185 in file startup_stm32f030x8.s
   Uses
      At line 86 in file startup_stm32f030x8.s
      At line 158 in file startup_stm32f030x8.s

FLASH_IRQHandler 00000012

Symbol: FLASH_IRQHandler
   Definitions
      At line 181 in file startup_stm32f030x8.s
   Uses
      At line 82 in file startup_stm32f030x8.s
      At line 154 in file startup_stm32f030x8.s

HardFault_Handler 0000000A

Symbol: HardFault_Handler
   Definitions
      At line 133 in file startup_stm32f030x8.s
   Uses
      At line 64 in file startup_stm32f030x8.s
      At line 134 in file startup_stm32f030x8.s

I2C1_IRQHandler 00000012

Symbol: I2C1_IRQHandler
   Definitions
      At line 198 in file startup_stm32f030x8.s
   Uses
      At line 102 in file startup_stm32f030x8.s
      At line 171 in file startup_stm32f030x8.s

I2C2_IRQHandler 00000012

Symbol: I2C2_IRQHandler
   Definitions
      At line 199 in file startup_stm32f030x8.s
   Uses
      At line 103 in file startup_stm32f030x8.s
      At line 172 in file startup_stm32f030x8.s

NMI_Handler 00000008

Symbol: NMI_Handler



ARM Macro Assembler    Page 3 Alphabetic symbol ordering
Relocatable symbols

   Definitions
      At line 128 in file startup_stm32f030x8.s
   Uses
      At line 63 in file startup_stm32f030x8.s
      At line 129 in file startup_stm32f030x8.s

PendSV_Handler 0000000E

Symbol: PendSV_Handler
   Definitions
      At line 141 in file startup_stm32f030x8.s
   Uses
      At line 75 in file startup_stm32f030x8.s
      At line 142 in file startup_stm32f030x8.s

RCC_IRQHandler 00000012

Symbol: RCC_IRQHandler
   Definitions
      At line 182 in file startup_stm32f030x8.s
   Uses
      At line 83 in file startup_stm32f030x8.s
      At line 155 in file startup_stm32f030x8.s

RTC_IRQHandler 00000012

Symbol: RTC_IRQHandler
   Definitions
      At line 180 in file startup_stm32f030x8.s
   Uses
      At line 81 in file startup_stm32f030x8.s
      At line 153 in file startup_stm32f030x8.s

Reset_Handler 00000000

Symbol: Reset_Handler
   Definitions
      At line 116 in file startup_stm32f030x8.s
   Uses
      At line 62 in file startup_stm32f030x8.s
      At line 117 in file startup_stm32f030x8.s

SPI1_IRQHandler 00000012

Symbol: SPI1_IRQHandler
   Definitions
      At line 200 in file startup_stm32f030x8.s
   Uses
      At line 104 in file startup_stm32f030x8.s
      At line 173 in file startup_stm32f030x8.s

SPI2_IRQHandler 00000012

Symbol: SPI2_IRQHandler
   Definitions
      At line 201 in file startup_stm32f030x8.s
   Uses
      At line 105 in file startup_stm32f030x8.s
      At line 174 in file startup_stm32f030x8.s



ARM Macro Assembler    Page 4 Alphabetic symbol ordering
Relocatable symbols


SVC_Handler 0000000C

Symbol: SVC_Handler
   Definitions
      At line 137 in file startup_stm32f030x8.s
   Uses
      At line 72 in file startup_stm32f030x8.s
      At line 138 in file startup_stm32f030x8.s

SysTick_Handler 00000010

Symbol: SysTick_Handler
   Definitions
      At line 145 in file startup_stm32f030x8.s
   Uses
      At line 76 in file startup_stm32f030x8.s
      At line 146 in file startup_stm32f030x8.s

TIM14_IRQHandler 00000012

Symbol: TIM14_IRQHandler
   Definitions
      At line 194 in file startup_stm32f030x8.s
   Uses
      At line 98 in file startup_stm32f030x8.s
      At line 167 in file startup_stm32f030x8.s

TIM15_IRQHandler 00000012

Symbol: TIM15_IRQHandler
   Definitions
      At line 195 in file startup_stm32f030x8.s
   Uses
      At line 99 in file startup_stm32f030x8.s
      At line 168 in file startup_stm32f030x8.s

TIM16_IRQHandler 00000012

Symbol: TIM16_IRQHandler
   Definitions
      At line 196 in file startup_stm32f030x8.s
   Uses
      At line 100 in file startup_stm32f030x8.s
      At line 169 in file startup_stm32f030x8.s

TIM17_IRQHandler 00000012

Symbol: TIM17_IRQHandler
   Definitions
      At line 197 in file startup_stm32f030x8.s
   Uses
      At line 101 in file startup_stm32f030x8.s
      At line 170 in file startup_stm32f030x8.s

TIM1_BRK_UP_TRG_COM_IRQHandler 00000012

Symbol: TIM1_BRK_UP_TRG_COM_IRQHandler
   Definitions



ARM Macro Assembler    Page 5 Alphabetic symbol ordering
Relocatable symbols

      At line 190 in file startup_stm32f030x8.s
   Uses
      At line 92 in file startup_stm32f030x8.s
      At line 163 in file startup_stm32f030x8.s

TIM1_CC_IRQHandler 00000012

Symbol: TIM1_CC_IRQHandler
   Definitions
      At line 191 in file startup_stm32f030x8.s
   Uses
      At line 93 in file startup_stm32f030x8.s
      At line 164 in file startup_stm32f030x8.s

TIM3_IRQHandler 00000012

Symbol: TIM3_IRQHandler
   Definitions
      At line 192 in file startup_stm32f030x8.s
   Uses
      At line 95 in file startup_stm32f030x8.s
      At line 165 in file startup_stm32f030x8.s

TIM6_IRQHandler 00000012

Symbol: TIM6_IRQHandler
   Definitions
      At line 193 in file startup_stm32f030x8.s
   Uses
      At line 96 in file startup_stm32f030x8.s
      At line 166 in file startup_stm32f030x8.s

USART1_IRQHandler 00000012

Symbol: USART1_IRQHandler
   Definitions
      At line 202 in file startup_stm32f030x8.s
   Uses
      At line 106 in file startup_stm32f030x8.s
      At line 175 in file startup_stm32f030x8.s

USART2_IRQHandler 00000012

Symbol: USART2_IRQHandler
   Definitions
      At line 203 in file startup_stm32f030x8.s
   Uses
      At line 107 in file startup_stm32f030x8.s
      At line 176 in file startup_stm32f030x8.s

WWDG_IRQHandler 00000012

Symbol: WWDG_IRQHandler
   Definitions
      At line 179 in file startup_stm32f030x8.s
   Uses
      At line 79 in file startup_stm32f030x8.s
      At line 152 in file startup_stm32f030x8.s




ARM Macro Assembler    Page 6 Alphabetic symbol ordering
Relocatable symbols

__user_initial_stackheap 00000014

Symbol: __user_initial_stackheap
   Definitions
      At line 225 in file startup_stm32f030x8.s
   Uses
      At line 223 in file startup_stm32f030x8.s
Comment: __user_initial_stackheap used once
34 symbols



ARM Macro Assembler    Page 1 Alphabetic symbol ordering
Absolute symbols

Heap_Size 00000200

Symbol: Heap_Size
   Definitions
      At line 44 in file startup_stm32f030x8.s
   Uses
      At line 48 in file startup_stm32f030x8.s
      At line 229 in file startup_stm32f030x8.s

Stack_Size 00000400

Symbol: Stack_Size
   Definitions
      At line 33 in file startup_stm32f030x8.s
   Uses
      At line 36 in file startup_stm32f030x8.s
      At line 228 in file startup_stm32f030x8.s

__Vectors_Size 000000B4

Symbol: __Vectors_Size
   Definitions
      At line 111 in file startup_stm32f030x8.s
   Uses
      At line 59 in file startup_stm32f030x8.s
Comment: __Vectors_Size used once
3 symbols



ARM Macro Assembler    Page 1 Alphabetic symbol ordering
External symbols

SystemInit 00000000

Symbol: SystemInit
   Definitions
      At line 119 in file startup_stm32f030x8.s
   Uses
      At line 120 in file startup_stm32f030x8.s
Comment: SystemInit used once
__main 00000000

Symbol: __main
   Definitions
      At line 118 in file startup_stm32f030x8.s
   Uses
      At line 122 in file startup_stm32f030x8.s
Comment: __main used once
__use_two_region_memory 00000000

Symbol: __use_two_region_memory
   Definitions
      At line 222 in file startup_stm32f030x8.s
   Uses
      None
Comment: __use_two_region_memory unused
3 symbols
387 symbols in table
